# Blackbody Radiation Lab

Brandon Lim

12/11/24

**Figure 1a.** Measured heat transfer in micro-watts on the x-axis versus theoretically calculated heat transfer in micro-watts on the y-axis. The blue markers represent experiment one, the red markers represent experiment 2, and the green markers represent experiment 3. The solid black line represents a one to one line to show where data points should be if theory and experimental values agree.

A graph showing a line

Description automatically generated with medium confidence

**Figure 1b.** Measured heat transfer in micro-watts on the y-axis versus reciprocal of squared distance from the source in inverse meters squared on the x-axis. The blue markers represent experiment one values and the black line represents a linear regression. The residuals squared is shown on the plot as well.

A graph showing a line

Description automatically generated with medium confidence

A diagram of a person with a line

Description automatically generated with medium confidence

A black and white diagram

Description automatically generated

**Figure 1d.** Measured heat transfer in micro-watts on the y-axis versus black body emission diameter squared in meters squared on the x-axis. The green markers represent experiment 3 data and the black line represents a linear regression. The residual squared value is also shown.

**Figure 1c.** Measured heat transfer in micro-watts on the y-axis versus blackbody temperature reported in Kelvin to the fourth power on the x-axis. The red markers represent experiment 2 data and the black line represents a linear fit line. The residual squared value is also shown.

Short-Answer Questions

A math problem with numbers and symbols

Description automatically generated

2a. The average percent relative difference for the agreement of measured and theoretical heat transfer across all experiments was 33.31%. These agreements seem to be better where the range was investigated as the diviation from the 1:1 line that matches theory with measurement grows at the end of the range.

A close up of black text

Description automatically generated

2b. Theory was an adequate assessment of where the heat transfer range would be but it was not completely accurate measurement. This can be seen in plot 1a where the 1:1 line is in close proximity to the data points but not exactly touching them.Theory also was also better at calculating different scenarios and experiments as we saw the residual square value get further away from one going down the experiments.

A text on a white background

Description automatically generated

2c. To find the unknown emissivity of the gray body, the data analysis portion of the experiment can be altered to solve for the unknown emissivity rather than theoretical parameters. This can be down by emitting a known heat transfer from the grey body and measuring it certain distances and criteria just like in this experiment. We then will have all the heat transfer values as seen in equation 14 of the handout with an addition epsilon term on the numerator (emmisivity) that we can solve for.