# Heat Exchanger Lab

Brandon Lim

12/1/2024

**Table 1a.** Characteristics table of the shell and tube heat exchanger experiment. The three left columns show different cases of hot and cold fluid flow rates in kilograms per second while the top row shows heat exchanger characteristics in SI units such as fluid temperature difference in degrees Celsius, overall heat transfer coefficient in watter per meter squared kelvin, and heat transfer rates in watts.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Case | Flow Rate (kg/s) | | Temperature (oC) | | Ui (W/Km2) | Heat Transfer Rate (kW) | | |
|  |  |  |  | qc | qh | (%) |
| 1a | 0.2395 | 0.2876 | 5.1667 | 6.7778 | 1973.45 | 6.8035 | 6.2106 | 9.1111 |
| 1b | 0.2332 | 0.1875 | 7.000 | 6.7778 | 1738.28 | 6.6250 | 5.4878 | 18.7762 |
| 2a | 0.2017 | 0.3250 | 4.000 | 7.1667 | 1705.01 | 6.0579 | 5.4346 | 10.8474 |
| 2b | 0.2143 | 0.1875 | 6.8889 | 7.0000 | 1684.43 | 6.2876 | 5.4000 | 15.1889 |

**Table 1b.** Characteristics table of the shell and tube heat exchanger experiment. The three left columns show different cases of hot and cold fluid flow rates in kilograms per second while the top row shows heat exchanger characteristics in SI units such as heat capacities, non-dimensional number of transfer units, and heat transfer effectiveness.

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Case | Flow Rate (kg/s) | | Cr | NTU |  | | |
|  |  | measured | Theory | (%) |
| 1a | 0.2395 | 0.2876 | 0.8351 | 0.2157 | 0.1785 | 0.1800 | 0.8649 |
| 1b | 0.2332 | 0.1875 | 0.8021 | 0.2432 | 0.1963 | 0.1995 | 1.6157 |
| 2a | 0.2017 | 0.3250 | 0.6222 | 0.2213 | 0.1855 | 0.1875 | 1.0977 |
| 2b | 0.2143 | 0.1875 | 0.8727 | 0.2357 | 0.1905 | 0.1931 | 1.3602 |

A comparison of a graph

Description automatically generated with medium confidence

**Figure 1c.** Zoomed out plot of theoretical curves of effectiveness on the y-axis and number of transfer units on the x-axis (Left). The blue circles represent calculated measured effectiveness and the black crosses represent calculated theoretical effectiveness. Zoomed in plot of theoretical curves of effectiveness on the y-axis and number of transfer units on the x-axis (Right).

Short-Answer Questions

**A close-up of a text

Description automatically generated**

2a. The range of percent differences for the heat transfer is 9.11% to 18.78%. The range of percent uncertainty in the calculated heat transfer rates is 4.92% to 5.52% and 6.22% to 7.15% for the cold fluid heat transfer and hot fluid heat transfer respectively. Collectively, the uncertainty in the measurements helps to explain the observed difference between qc and qh because the max percent uncertainty for each respectively is 5.52% and 7.15%. This max difference leads to discrepancies in actual physical phenomena and our recorded data which can explain the discprepancy between the hot fluid heat transfer and the cold fluid heat transfer.

A close-up of a text

Description automatically generated

The percent differences in effectiveness obtained in the measurements compared to theory are 0.86%, 1.62%, 1.10%, and 1.36% for flow case 1, case 2, case 3, and case 4 respectively. The theory does adequately describe the observations because of such a low percent difference between the values. It is possible to use theory to predict the effectiveness of flow rates of 0.3 kg/s for the cold fluid and 0.4kg/s for the hot fluid. This is because these flow rates are close to or within range of the experimental flow rates used to find the low percent difference in effectiveness. Therefor, we can reliably assume that these flow rates would have similar behavior to the experimental conclusions.

A close-up of a text

Description automatically generated

2c. [insert your response here]